## Introduction

This device is intended for users who have difficulty removing the seal on a canned jar.

## Features

Diagram

Description automatically generated

## Usage

To use the device on a two part mason jar lid, place the bump on the end on the lid of the jar after the outer ring has been removed, and place the hook under the edge of the lid. Lever the handle of the device upwards and the lid will come off. For a one piece lid, follow the same procedure, this will allow air into the jar so the lid can be removed easier.

## Compatibility

This is compatible with mason jars with two part lids, as well as one part twist off lids.

## Specifications

Length:150mm

Width:50mm

Weight:25g

## Cleaning

The device can be wiped clean with a damp cloth